Freq=1MHz F=10MHz

A(10,10)\*B(10,10) => operations number = 10^3=1000 multiplications

1 multiplication => 10clocks => 1sec =>100 000multiplications

Execution time = 1000\*10clocks/1000000clocks/sec=0.01 sec =>0.001 sec on 10 MHz computer