**EASTERN MEDITERRANEAN UNIVERSITY**

**COMPUTER ENGINEERING DEPARTMENT**

**CMPE224 DIGITAL LOGIC SYSTEMS**

**EXPERIMENTAL WOK #3**

**REGISTERS IN VeriLog HDL**

**OBJECTIVES:**

This laboratory work aims to introduce a practical work on the design of Registers from architectural and behavioral descriptions. The architectural description covers both the schematic and the software implementation of circuits designed through the conventional design procedure. The behavioral descriptions cover the implementation using state transition diagrams.

**Important Note:** *For each of the following experimental tasks (in each phase), open a new project to avoid compilation errors due to multiple use of components within the same project’s files.*



**Phase 1: Schematic-Entry**


Assume that we want to design the following multi-function register that is controlled by two control inputs S1 and S0 as follows:


|  |  |  |
| --- | --- | --- |
| **Mode Control** | | **Register**  **Operation** |
| ***S1*** | ***S0*** |
| 0 | 0 | *No change* |
| 0 | 1 | *Shift left* |
| 1 | 0 | *Shift right* |
| 1 | 1 | *Parallel Load* |

The schematic circuit corresponding to this multi-function register is given below:

* 1. Draw the circuit of this multifunction register, compile and simulate it in VeriLog HDL environment and verify its mode of operations. Adjust and apply appropriate waveforms to observe different function modes easily.







**Phase 2: Implementing the Architectural Design of Multi-Function Register in Verilog HDL**

Enter the following architectural VeriLog code of multifunction register design into Quartus Lite development suite. Compile and simulate your code to verify its correctness.

/\* 4-bit Multifucntion Register controlled by two control inputs S1 and S0 as follws:

s1 s0=00 No change

01 Shift left

10 Shift right

11 Parallel load

\*/

module MultiFuncRegister\_Arch(Clear,CLK,S,PL,IL,IR,Q);

input CLK;

input Clear;

input IL, IR; // Serial load from left and right

input [1:0] S; // Vector of control inputs S1 and S0

input [3:0] PL; // Parallel load

output [3:0] Q; // Register ouputs Q3, Q2, Q1, Q0

wire [3:0] W; // Internal signals among components

MUX\_4\_1 m1(W[0],S[1],S[0],PL[0],IL,Q[1],Q[0]);

MUX\_4\_1 m2(W[1],S[1],S[0],PL[1],Q[0],Q[2],Q[1]);

MUX\_4\_1 m3(W[2],S[1],S[0],PL[2],Q[1],Q[3],Q[2]);

MUX\_4\_1 m4(W[3],S[1],S[0],PL[3],Q[2],IR,Q[3]);

D\_FF d1(Q[0],W[0],CLK,Clear);

D\_FF d2(Q[1],W[1],CLK,Clear);

D\_FF d3(Q[2],W[2],CLK,Clear);

D\_FF d4(Q[3],W[3],CLK,Clear);

endmodule

module D\_FF(Q,D,CLK,CLR);

input D,CLK,CLR;

output reg Q;

always @(posedge CLK)

if (CLR == 1'b1)

Q<= 1'b0;

else

Q<= D;

endmodule

module MUX\_4\_1(Y,S1,S0,I3,I2,I1,I0);

input S1,S0,I3,I2,I1,I0;

output reg Y;

always @(S1,S0,I3,I2,I1,I0)

begin

if (S1==0 & S0==0)

Y=I0;

else if (S1==0 & S0==1)

Y=I1;

else if (S1==1 & S0==0)

Y=I2;

else if (S1==1 & S0==1)

Y=I3;

end

endmodule

**HOMEWORK #3 : (Behavioral Description of a Multi-funtion Regiter)**

Behavioral VeriLog code of the above described multifunction register is given below:

/\* Behavioral description of a multifunction register in veriLog HDL

s1 s0 =00 Nocahnge

S1 S0 =01 Shift left

S1 S0 =10 Shift right

S1 S0 =11 Parallel load

\*/

module MultiFunctRegister\_Behav(Clear,CLK,S,PL,IL,IR,Q);

input Clear, CLK;

input [3:0] PL;

input [1:0] S;

input IL,IR;

output [3:0] Q;

reg [3:0] R;

always @(posedge CLK)

begin

if (Clear == 1)

R <= 4'b0000;

else if (S[1]==0 & S[0]==0) // No change

R <= R;

else if (S[1]==0 & S[0]==1) // Shift left

begin

R[0] <= IR; R[1] <= R[0];

R[2] <= R[1]; R[3] <= R[2];

end

else if (S[1]==1 & S[0]==0) // Shift right

begin

R[3] <= IL; R[2] <= R[3];

R[1] <= R[2]; R[0] <= R[1];

end

else if (S[1]==1 & S[0]==1)

begin

R=PL;

end

end

assign Q = R;

endmodule

Modify the above-given behavioral code to design a 4-bit multifunction register that operates as follows:

**Enable S1 S0 Operation Mode**

*0 x x No change*

*1 0 0 Rotate left*

*1 0 1 XOR contents with (0101)*

*1 1 0 Rotate right*

*1 1 1 Parallel load*

Submit your homework at the beginning of the 4-the experimental work.

*Prepared by Assoc. Prof. Dr. Adnan ACAN*